00000000000i[     ] Bochs x86 Emulator 2.2.1
00000000000i[     ]   Build from CVS snapshot on July 8, 2005
00000000000i[     ] System configuration
00000000000i[     ]   processors: 1
00000000000i[     ]   A20 line support: yes
00000000000i[     ]   APIC support: yes
00000000000i[     ] CPU configuration
00000000000i[     ]   level: 6
00000000000i[     ]   fpu support: yes
00000000000i[     ]   paging support: yes, tlb enabled: yes
00000000000i[     ]   mmx support: yes
00000000000i[     ]   sse support: 1
00000000000i[     ]   v8086 mode support: yes
00000000000i[     ]   3dnow! support: no
00000000000i[     ]   PAE support: yes
00000000000i[     ]   PGE support: yes
00000000000i[     ]   PSE support: yes
00000000000i[     ]   x86-64 support: no
00000000000i[     ]   SEP support: no
00000000000i[     ] Optimization configuration
00000000000i[     ]   Guest2HostTLB support: yes
00000000000i[     ]   RepeatSpeedups support: yes
00000000000i[     ]   Icache support: yes
00000000000i[     ]   Host Asm support: yes
00000000000i[     ]   Fast function calls: yes
00000000000i[MEM0 ] allocated memory at 00B40020. after alignment, vector=00B41000
00000000000i[MEM0 ] 32.00MB
00000000000i[MEM0 ] rom at 0xf0000/65536 ('c:\progra~1\bochs\BIOS-bochs-latest')
00000000000i[MEM0 ] rom at 0xc0000/32768 ('c:\progra~1\bochs\VGABIOS-elpin-2.40')
00000000000i[APIC?] local apic in  initializing
00000000000i[APIC?] set APIC ID to 0
00000000000i[APIC0] 80686
00000000000i[APIC0] local apic in CPU apicid=00 initializing
00000000000i[IOAP ] initializing I/O APIC
00000000000i[IOAP ] set APIC ID to 1
00000000000i[CMOS ] Using local time for initial clock
00000000000i[CMOS ] Setting initial clock to: Sun Nov 20 23:53:02 2005 (time0=1132548782)
00000000000i[DMA  ] channel 4 used by cascade
00000000000i[DMA  ] channel 2 used by Floppy Drive
00000000000i[FDD  ] fd0: 'floppy.img' ro=0, h=2,t=80,spt=18
00000000000i[WGUI ] Number of Mouse Buttons = 5
00000000000i[WGUI ] IME disabled
00000000000i[CLVGA] VBE Bochs Display Extension Enabled
00000000000i[CLVGA] interval=300000
00000000000i[CLVGA] CL-GD5430 ISA initialized
00000000000i[     ] init_mem of 'harddrv' plugin device by virtual method
00000000000i[     ] init_mem of 'keyboard' plugin device by virtual method
00000000000i[     ] init_mem of 'serial' plugin device by virtual method
00000000000i[     ] init_mem of 'parallel' plugin device by virtual method
00000000000i[     ] init_mem of 'extfpuirq' plugin device by virtual method
00000000000i[     ] init_mem of 'gameport' plugin device by virtual method
00000000000i[     ] init_mem of 'speaker' plugin device by virtual method
00000000000i[     ] init_dev of 'harddrv' plugin device by virtual method
00000000000i[HD   ] Using boot sequence floppy, none, none
00000000000i[HD   ] Floppy boot signature check is enabled
00000000000i[     ] init_dev of 'keyboard' plugin device by virtual method
00000000000i[KBD  ] will paste characters every 1000 keyboard ticks
00000000000i[     ] init_dev of 'serial' plugin device by virtual method
00000000000i[SER  ] com1 at 0x03f8 irq 4
00000000000i[     ] init_dev of 'parallel' plugin device by virtual method
00000000000i[PAR  ] parallel port 1 at 0x0378 irq 7
00000000000i[     ] init_dev of 'extfpuirq' plugin device by virtual method
00000000000i[     ] init_dev of 'gameport' plugin device by virtual method
00000000000i[     ] init_dev of 'speaker' plugin device by virtual method
00000000000i[     ] reset of 'harddrv' plugin device by virtual method
00000000000i[     ] reset of 'keyboard' plugin device by virtual method
00000000000i[     ] reset of 'serial' plugin device by virtual method
00000000000i[     ] reset of 'parallel' plugin device by virtual method
00000000000i[     ] reset of 'extfpuirq' plugin device by virtual method
00000000000i[     ] reset of 'gameport' plugin device by virtual method
00000000000i[     ] reset of 'speaker' plugin device by virtual method
00000004447i[BIOS ]  rombios.c,v 1.138.2.1 2005/07/06 19:30:36 vruppert Exp $
00000318308i[KBD  ] reset-disable command received
00000600000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00004366874e[HD   ] device set to 0 which does not exist
00004367167e[HD   ] device set to 1 which does not exist
